CP210x USB to UART Bridge VCP Drivers

The CP210x USB to UART Bridge Virtual COM Port (VCP) drivers are required for device operation as a Virtual COM Port to facilitate host communication with CP210x products. These devices can also interface to a host using the USBXpress direct access driver.

Download for Windows XP/Server 2003/Vista/7 (v6.5.3)

The CP210x Manufacturing DLL and Runtime DLL have been updated and must be used with v6.0 and later of the CP210x Windows VCP Driver. Application Note Software downloads affected are AN144SW.zip, AN205SW.zip and AN223SW.zip. If you are using a 5.x driver and need support you can download archived Application Note Software. 

· VCP Driver Kit
· Revision History
· USB Driver Installation Utility Application Note, AN335
· USB Driver Installation Utility Software, AN335SW
Download for Windows 2K (v6.3a)

· VCP Driver Kit
· Revision History
Download for WinCE

· VCP Driver for WinCE 6.0 (2.1)
· VCP Driver for WinCE 6.0 Revision History
· VCP Driver for WinCE 5.0 (2.1)
· VCP Driver for WinCE 5.0 Revision History
Download for Macintosh OSX (v3.0)

· VCP Driver Kit
· Revision History
Download for Linux (2.6.x and 2.4.36)

· VCP Driver Kit
· Revision History
