Description Of Frequency Determining And Stabilizing Circuit Introduction

The frequencies for transmitter and receiver local frequencies are all derived  a signal 4.5 [MHz] crystal by means of a phase locked loop. The first local oscillator frequencies are 16.27 [MHz] (CH.1) to 16.71 [MHz] (CH.40). The second local frequency is fixed at 10.240 [MHz] to generate second IF 455 [KHz]. During transmit, the VCO of the PLL operates 13.4825[MHZ] (CH.1) to 13.7025 [MHz] (CH.40). The VCO  frequency goes to the doublers circuit Q301, L301, L302 which  doublers the frequency to generate 26.965 [MHz] (CH.1) to 27.405 [MHz] (CH.40).


                                                                                               To Transmitter


13.4825[MHz] (CH.1)                                          26.965 [MHz] (CH.1)

                        ~ 13.7025 [MHz] (CH.40)                                     ~27.405 [MHz] (CH.40)                                                  
The VCO operating frequency for the receiver is 16.27 [MHz] (CH.1) to 16.71 [MHz] (CH.40) as the first local oscillator, injected through the buffer amp Q506 into the first FET balanced mixer Q107, Q108 

Descriptions Of Each Block

1. Introduction

The synthesizer is implemented with the following
Components : PLL IC (IC6)



            X-TAL  (X401)



           VCO, Varicap Diode (D503,504)

       IC101 is a MCU that includes LCD driver and all of control circuit.

       The PLL IC (IC6) of PLL block, 

The Q503, L404, C511, C512, C513, C507,Varicap diode D503 and D504 are clap oscillator   

circuit to operate as a VCO.
The Q505 is a switching transistor to turn on or turn off the tuning  capacitor in the VCO       

oscillator tank circuit for transmitter or receiver. The Q506 works as a buffer amp for  RX  

local frequencies (16 [MHz]) and TX carrier generating frequencies (13 [MHz]).
   2. Reference Frequency

The crystal, X401(4.5 [MHz]) and other components at pin1 and 16 of  IC6 can make a   

reference frequency oscillator with internal amplifier.

2-1. VCO

The Q503 and surrounding parts are consisting a clap oscillator work as a VCO of IC6 with 
appropriate control voltage on D503 and D504, the can be oscillate over the required range 

of  13.4825[MHz] to 16.71 [MHz].
2-2. Programmable Divider And PLL Data Control

The MCU(IC101)  and PLL IC (IC6) communicate by serial data for PLL IC data setting.
The programmable inputs for each channels set by MCU (IC101). Each input signal to 

control the PLL IC is done with the provided key input pins 20 and 21  of IC101.  

2-3. Phase Detector And VCO Control

The phase detector is a digital phase comparator which compares the phase of the reference  

signal with programmable divider output square waves and develops a series of pulses   

whose DC level depends on the phase error of each signal. 

The phase detector pulse output is fed to an active low pass filter and RC low pass filter 

output signal of IC6 is filtered and fed to varicap  D503 and 504 control the VCO frequency.
TRANSMITTER / RECEIVER BUFFER AMP

Output signal of Q503 is fed into the buffer AMP Q506, L401 to increase the  strength of  TX  

carrier frequency and 1st local frequencies.
Transmitter Doublers
The output signal of Q506, L401 goes to an amplifier with tuning circuit Q301, L301, L302 which doubles incoming 13 MHz signals.
Switching Of Tuning Capacitor In VCO

The VCO circuit must tune with a wide range of frequencies 13.4825 ~ 13.7025 [MHz] for  

transmitter and 16.27 ~ 16.710 [MHz] for receiver. To comply above range of  VCO, the   

tuning Capacitance should switched for transmission or reception.
The tuning circuit consists with L401, C507, C512, C513, C522, when the VCO is working  

as a receiver Q505 becomes turn off.  So, L401 AND  D503,504 makes tuning function.

When transmitting Q505 becomes on. So, L401 and the parallel capacitance of C522 and  

D503,504 make turning function.

Receiver Local Oscillator  outputs
1ST mixer : The secondary output signals of  L401 is injected to the source of 1ST mixer  

                 Q107,Q108 in the 1ST IF mixer section.

2ND mixer : The output of 10.24 [MHz] oscillator circuit with X1 is injected into the IF module (IC102) . Incoming IF signal and 10.24 [MHz] signal are mixed inside the  IF IC to extract 2ND IF signal 455 [MHz]. FM and AM signals are recovered with envelope detector.
         Frequency Stability     

         Let : Fo = Crystal Oscillator Frequency 

                 Fr =  Phase Detector Reference Frequency 

                 Fvco = VCO Frequency

                 Ft = Transmit Frequency 

                 Then : Fr = Fo/1800

                 And under locked conditions : Fr = Fvco / N

                 Where , “N” is the programmable divider ratio.

         Then : Fvco = N X Fr 

         From which it can be seen, the percentage error in  Ft is the same as percentage error in Fo.
         The stability of the crystal oscillator is determined  primarily by the itself and having passive 

         components  of the oscillator.
         The choice of crystal and components is such that the required frequency stability is       

          maintained over the required voltage and temperature range.

Description Of Transmitter And Receiver

1. The Transmitter

   RF Amplification
The output of doublers AMP Q301 is fed through tuning IFT  L301 and L302 to the base of 
pre-driver  AMP Q305. 

The output is then supplied through tuning circuit L303 to RF driver AMP  Q306. 
The output of Q306 is supplied with tuning circuit L304, C321, RFC306 and goes to the base of     

final  RF AMP Q307. The output of Q307 is supplied to the antenna through  L-C tuning circuit.

   CIRCUIT FOR SUPPRESSION  OF SPURIOUS RADIATION

The  tuning circuit between the output of final AMP Q303 and antenna,    7-stage  “LPF”  

network L310, C331, C332, L311, C333, C335, L312, C337, 
serves as a  spurious radiation suppressor.  This network also serves to match the  

impedance between TX power AMP Q307 and the antenna. 

   Circuits For Limiting Power

After finished  all alignment, to constant voltage supply circuit limits the available power 4 [W] or  

slightly less. RV-203 and corresponding three transistors control supply voltage of  RF amplifier 

and other circuits.

Tune all the trimming parts for maximum indication of RF power meter and adjust RV-203 to  

make 4 [W] indication of RF power meter. The tuning is adjusted so that the actual power is 
from 3.8 to 4.0 [W]. There are on other additional controls for adjusting the TX output power.
   Max Deviation Control

   The deviation signals are filtered with RC network and goes to the OP  AMP IC IC3 make 

   nominal signal level to achieve wanted modulation.    To control incoming audio signal, diode

   D451,452 and corresponding limiter circuit controls with proportional to sampled audio output   

   level adjust RV501 shall not exceed  (2[KHz] max deviation under 1.25 [KHz] AF 20 dB up from 
   1kHz modulation level input.

Max Modulation Control

The modulation signal are filtered with RC network and goes to the audio AMP IC IC104 make amplitude signal to achieved AM modulation. 

To control incoming audio signal, diode D202, Q208, and Q207  corresponding limiter circuit

controls with proportional to sampled audio output level adjust by RV201 shall not exceed 100% max modulation under 60% AF 20dB up from 1KHz modulation input.

2. The RECEIVER

    RF AMP Q104 amplify RF signal from antenna, the amplified RF SIGNAL is fed through tuning    

coils L102, L103 to the gate of  double balance mixer FET, Q107, Q108 also  VCO sources  

frequency lower 10.695 MHz than the frequency of each channel is supplied to mixer.
    The source of 10.695MHz frequency filtered by CF1 is fed to through  to IC102.

    The 455KHz frequency signal produced from IC102 by mixing the output source of CF1   

      10.695MHz filter and the source of 10.240MHz frequency from crystal oscillator X1.

     Internal AM and FM detector of IC102 detect AM and FM audio signal.

     A.G.C(Automatic Gain Control) signal of  IC102 fed to IC103, D122, Q121 control receiving  

      sensitivity.

     The AM detected audio signals fed through R157, C167, D151, VR101 to low frequency audio   

        AMP for driving speaker.

The FM audio detected and amplified audio signal is fed through high cut filter R161, C153,  

  D152,VR101 to speaker.
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