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	Reading Point
	Adjustment
	Description
	Value

	TP1
	CT1
	Band A -80 Ch.
	19.655MHz

	TP1
	CT2
	Band B -40 Ch.
	19.880MHz

	TP1
	CT3
	Band C CEPT
	20.105MHz

	TP1
	CT4
	Band D + 40 Ch.
	20.330MHz

	TP1
	CT12
	Band E + 80 Ch.
	20.555MHz

	TP1
	CT5
	Band C CEPT
	20.1035MHz

	TP2
	T1
	0utput to RF local oscillator
	37.660-38.100MHz for CEPT

	TP3
	VCO-Coil
	VCO DC Voltage
	2,5 Volt @ 27.175MHz

	TP4
	CT11
	AM
	10.695MHz

	TP4
	CT10
	LSB
	10.692MHz



	Adjustment
	Description
	Value

	RECEIVER
	 
	 
	 

	T8
	RF Input
	 
	

	T9
	RF Input
	 
	

	T10
	RF Input
	 
	

	T11
	1. IF
	10,7MHz
	

	T12
	1. IF
	10,7MHz
	

	T13
	AM IF
	455kHz
	

	T14
	AM Detector
	455kHz
	

	T6
	SSB IF
	455kHz
	

	T7
	SSB Detector
	 
	

	T16
	FM Discriminator
	 
	

	TRANSMITTER
	 
	 
	 

	T1
	PLL Output to Converter
	37.660 - 38.100MHz for CEPT
	

	T2
	PLL Output to Converter
	37.660 - 38.100MHz for CEPT
	

	T3
	Transmitter Output
	26.965 - 27.405MHz for CEPT
	

	T4
	Transmitter Output
	26.965 - 27.405MHz for CEPT
	

	T5
	Transmitter Output
	26.965 - 27.405MHz for CEPT
	

	L16
	Transmitter Output
	26.965 - 27.405MHz for CEPT
	

	CT8
	Transmitter Output USB/LSB
	26.965 - 27.405MHz for CEPT
	

	CT9
	Transmitter Output USB/LSB
	26.965 - 27.405MHz for CEPT
	

	RV2
	Bias Q8
	 
	

	RV11
	AM/FM Output Power
	10 Watt
	

	METER
	 
	 
	 

	RV4
	RF Power Meter
	 
	

	RV8
	RF S-Meter
	SSB (USB/LSB)
	

	RV9
	RF S-Meter
	AM/FM
	

	.
	 
	 
	 

	RV1
	FM Modulation
	+/- 2kHz
	

	RV6
	SSB Modulation
	18 Watt p-p
	

	RV11
	AM Modulation
	90%
	

	RV5
	Carrier at SSB
	Adjust for NO Carrier
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