ALAN 48 PLUS MULTI B

MODIFICATION TO OPERATION 400CH AND OTHERS BAND ON ALAN 48 PLUS MULTI B

- Open the radio and remove screw cap.
- Look for the three jumper OPT1,OPT2,OPT3, see you the photo
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Selection the Band
- Power off the radio;

- Keep and hold the buttons ‘AM/FM’ and ‘SCAN’ then power on the radio.
- Turn the knob ‘CHANNEL’ and to select the band.

- Push the button ‘AM/FM’ to finish the selection.

TRIMMER LAYOUT MODULATION LEVEL AM/FM
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To increase the modulation and deviation to turn the trimmer in an anticlockwise

-RV901 AM modulation level trimmer

-RV301 FM deviation level trimmer
