MODIFICA POTENZA E BANDE SU MIDLAND G7 XT
POWER OUTPUT AND BAND SETTING ON MIDLAND G7 XT
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Italiano:
Rimuovete le viti lato pacco batterie,aprite la radio ed individuate i ponticelli come riportato sopra,  scegliete uno delle seguenti configurazioni:
Per personalizzare il menù della vostra radio:
	JP1
	JP2
	JP3
	SETAGGI

	
	
	
	PMR
	LPD

	0
	0
	0
	/
	LPD 10mW

	0
	0
	1
	/
	*LPD 3W(H)  (L)500mW  

	0
	1
	0
	PMR (H) 500mW  (L) 10mW condizione impostata in fabbrica
	LPD 10mW condizione impostata in fabbrica

	0
	1
	1
	PMR (H) 3W          (L) 500mW
	LPD 500mW

	1
	0
	0
	PMR (H) 500mW  (L) 10 mW
	/

	1
	0
	1
	PMR (H) 3W          (L) 500mW
	/

	1
	1
	0
	PMR (H) 500mW  (L) 10mW
	LPD Menu(H) 500mW  Menu(L) 10mW

	1
	1
	1
	PMR (H) 3W          (L) 500mW
	LPD Menu(H) 3W          Menu(L) 500mW


*Questa funzione  è disponibile prossimamente,per il momento è disponibile solamente a 500mW.Per avere 3W anche in LPD usare la combinazione 111.
 0=CHIUSO               

 1=APERTO

H= ALTA POTENZA

L= BASSA POTENZA
English:

Remove the screws side package batteries, open the radio and look for the jumper (see you above picture),below you have all kind of configurations:
	JP1
	JP2
	JP3
	SETTING

	
	
	
	PMR
	LPD

	0
	0
	0
	/
	LPD 10mW

	0
	0
	1
	/
	*LPD 3W(H)  (L)500mW  

	0
	1
	0
	PMR (H) 500mW  (L) 10mW default setting
	LPD 10mW default setting 

	0
	1
	1
	PMR (H) 3W          (L) 500mW
	LPD 500mW

	1
	0
	0
	PMR (H) 500mW  (L) 10 mW
	/

	1
	0
	1
	PMR (H) 3W          (L) 500mW
	/

	1
	1
	0
	PMR (H) 500mW  (L) 10mW
	LPD Menu(H) 500mW  Menu(L) 10mW

	1
	1
	1
	PMR (H) 3W          (L) 500mW
	LPD Menu(H) 3W          Menu(L) 500mW


*This option is available sooner, now there is only at 500mW 
0=CLOSE
1=OPEN

H=HIGHT POWER

L=LOWER POWER

