AE 6490 Microphone sensitivity Issue

Truck drivers report that MIC sensitivity is slightly too high.

Engine and traffic noise can be heard, especially in FM.

The problem can be solved by adding a resistor 4.7 kOhm  parallel to C 95:

[image: image1.jpg]312K £CO 100
3z, L
- oS & B
=i 2d,dgdgd2 insert 4.7k/Ohm
5525833 "3
I J «— Py
EC o
e
| 1 1
Ri00
2
ot
)01
7777
& oo sion
a0 oo S

> wew




Note: Please note that there is a drawing and part insertion error with C 93.

C 93 is wrong inserted and the drawing and silk printing is also wrong.

The + side must  be on the right side towards R 100 and not to the left side towards MIC_G_IN.

For Albrecht AE 6490  model this error does not matter anything, because there is no MIC gain potentiometer installed which could cause capacitor leakage current at this wrong polarity.

In next production you should insert the capacitor correctly and place the resistor 4.7 k between the junction point of   MIC_G_IN / MIC G-OUT  and ground

See here for next production running change:
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