take off bottom cover, to the right of the squelch is a long line of resistors and ONE blank one at the end. Bridge this with solder 25610-30110, A channels and others, bands rU,PX,RC,PC are unlocked
