ALAN 78 PLUS MULTI B

MODIFICATION TO OPERATION 400CH AND OTHERS BAND ON ALAN 78 PLUS MULTI B

- Open the radio and remove screw cap.
- Look for the three jumper OPT1,OPT2,OPT3, see you the photo
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Selection the Band
- Power off the radio;

- Keep and hold the buttons ‘AM/FM’ and ‘SCAN’ then power on the radio.
- Turn the knob ‘CHANNEL’ and to select the band.

- Push the button ‘AM/FM’ to finish the selection.

To increase AM Modulation in TX.
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Adjusting RV201counterclockwise to increase AM modulation.

To increase FM modulation adjusting RV401
