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Hinweis zur Anleitung AE 5290

Leider ist , bedingt durch einen bedauerlichen Übertragungsfehler, eine 

Funktion beschrieben, die in dem Gerät nicht eingebaut ist.

Der Suchlauf über die Memorykanäle, wie auf Seiten 14/15 beschrieben, ist in 

diesem Gerät nicht vorhanden. Die korrigierte Bedienungsanleitung finden Sie auf unserem Downloadserver unter http://www.hobbyradio.de/CB/AE5290-Oct2005

Eine spezielle Anleitung für die 40 Kanal FM-CEPT Version

AE 5290 FM

finden Sie auf http://www.hobbyradio.de/CB/AE5290FM

Nur diese Version ist zum Betrieb in Österreich zugelassen!

[image: image2.jpg]& ALBRECHT.




Annex to User Manual AE 5090

We regret a transfer error in the user manual of AE 5090.

The described Memory Scan function (page 13) is not implemented in this model.

You may download the corrected user manual from our server under

http://www.hobbyradio.de/CB/AE5290-Oct2005
Our special user manual for the 40 CH FM  (CEPT) version 

AE 5290 FM

can be downloaded from 

http://www.hobbyradio.de/CB/AE5290FM

Only this version is allowed for use in Austria.

