MODIFICATIE POLMAR DB-32
here below you can find the procedure:

-------------------------------

1)Pls long time press "MENU",and power on,The LCD display "RESET".

2)Then press again"MENU",the LCD display"VFO",press  "UP" keypad to "BAND".

3)Then press"MENU",the LCD display "PSWD",press "5858",the LCD display

"BAND1"frequency is 144-146,you input 136-174.

4)Then press  "UP" keypad,the LCD display "BAND2"frequency is 430-440,you input 400-470.Then press"MENU" to confirm exit.then re-power on,and you can use the new setting frequency.

